*Heading
** Job name: Job-1 Model name: Model-1
** Generated by: Abaqus/CAE 6.10-2
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=Part-1
*End Part
**
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Part-1-1, part=Part-1
*Node
*Element, type=S8R5
*Nset, nset=_PickedSet2, internal, generate
*Elset, elset=_PickedSet2, internal, generate
** Section: Section-1
*Shell General Section, elset=_PickedSet2
817036., 35937.6, 817036., 0., 0., 44737.2, 0., 0.
0., 8.56e+06, 0., 0., 0., 311579., 5.61e+06, 0.
0., 0., 0., 0., 387872.,
*Transverse Shear
*End Instance
**
*Nset, nset=_PickedSet5, internal, instance=Part-1-1
*Elset, elset=_PickedSet5, internal, instance=Part-1-1
*Nset, nset=_PickedSet6, internal, instance=Part-1-1
*Elset, elset=_PickedSet6, internal, instance=Part-1-1, generate
*Nset, nset=_PickedSet7, internal, instance=Part-1-1
*Elset, elset=_PickedSet7, internal, instance=Part-1-1, generate
*Elset, elset=__PickedSurf4_E2, internal, instance=Part-1-1, generate
*Elset, elset=__PickedSurf4_E3, internal, instance=Part-1-1, generate
*Surface, type=ELEMENT, name=_PickedSurf4, internal
__PickedSurf4_E2, E2
__PickedSurf4_E3, E3
*End Assembly
**
** BOUNDARY CONDITIONS
**
** Name: BC-1 Type: Displacement/Rotation
*Boundary
_PickedSet5, 3, 3
** Name: BC-2 Type: Displacement/Rotation
*Boundary
_PickedSet6, 1, 1
** Name: BC-3 Type: Displacement/Rotation
*Boundary
_PickedSet7, 2, 2
** ----------------------------------------------------------------
**
** STEP: Step-1
**
*Step, name=Step-1, perturbation
*Buckle
10, , 10, 70
**
** BOUNDARY CONDITIONS
**
** Name: BC-1 Type: Displacement/Rotation
*Boundary, op=NEW, load case=1
_PickedSet5, 3, 3
*Boundary, op=NEW, load case=2
_PickedSet5, 3, 3
** Name: BC-2 Type: Displacement/Rotation
*Boundary, op=NEW, load case=1
_PickedSet6, 1, 1
*Boundary, op=NEW, load case=2
_PickedSet6, 1, 1
** Name: BC-3 Type: Displacement/Rotation
*Boundary, op=NEW, load case=1
_PickedSet7, 2, 2
*Boundary, op=NEW, load case=2
_PickedSet7, 2, 2
**
** LOADS
**
** Name: Load-1   Type: Shell edge load
*Dsload
_PickedSurf4, EDNOR, 1.
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field, variable=PRESELECT
*End Step